The SSG installation manual using INLINE installation scheme

Install and run Stingray Service Gateway, please refer to the installation requirements.

Set an IP address.

Apply for license installation and fastDPI to Service Desk.

Once installed both, you should edit the following settings into etc/dpi/fastdpi.conf:

Network packet transit configuration:

in_dev=dna0 out_dev=dna1 #Scale factor is about 1 for every 1 Gigabit of bandwidth scale_factor=10 timeout_check_dev=0 #FDPI Control ctrl_port=29000 ctrl_dev=lo #Turn on UDP detection only_tcp=0 #Turn on UDR udr=1

Statistics gathering:

http_parse_reply=1 netflow=8 netflow_full_collector_type=2 netflow_dev=eth3 netflow_timeout=20 netflow_full_collector=172.18.254.124:1500 netflow_rate_limit=30 netflow_passive_timeout=40 netflow_active_timeout=120 #URL upload ipfix_dev=eth3 ipfix_tcp_collectors=172.18.254.124:1501 ipfix_observation=127 #SIP ipfix_meta_tcp_collectors=172.18.254.124:1511 rlimit_fsize=32000000000

Further settings are made depending on components you plan to use and are listed in Section 3 in accordance with component's description.