The SSG installation manual using INLINE installation scheme

Prepare the server according to the installation requirements.

Install and configure the VEOS OS

Set an IP address.

Apply for license installation and fastDPI to Service Desk.

After installing them, the following settings must be made in etc/dpi/fastdpi.conf:

Set up transit:

in_dev=01:00.0 out_dev=01:00.1 #Scale factor is about 1 for every 1 Gigabit of bandwidth scale_factor=10 timeout_check_dev=0 #FastDPI Control ctrl_port=29000 ctrl_dev=lo #Turn on UDR udr=1

Statistics gathering:

#FullNetflow/IPFIX netflow=8 netflow_full_collector_type=2 netflow_dev=eth3 netflow_timeout=20 netflow_full_collector=172.18.254.124:1500 netflow_rate_limit=30 netflow_passive_timeout=40 netflow_active_timeout=120 #ClickStream/IPFIX ipfix_dev=eth3 ipfix_tcp_collectors=172.18.254.124:1501 #SIP ipfix_meta_tcp_collectors=172.18.254.124:1511 rlimit_fsize=32000000000

Further settings are made depending on which components are to be used. The settings are described in the SSG components section.