The SSG installation manual using on-stick installation scheme

Full description of on-stick mode in Configuring on-stick and LAG/LACP section

Prepare the server according to the installation requirements.

Install and configure the VEOS OS

Set an IP address.

Apply for license installation and fastDPI to Service Desk.

After installing them, the following settings must be made in etc/dpi/fastdpi.conf:

dpdk_device=port1:pci:86:00.0 dpdk_device=port2:pci:86:00.1 lag { name=LACP device=86-00.1 device=86-00.0 lacp=1 system_id=6c:b3:11:60:fa:66 priority=32768 balance_algo=0 } onstick_device { base=port1 filter=vlan(101,102) | qinq subs=subs1 inet=inet1 } onstick_device { base=port2 filter=vlan(101,102) | qinq subs=subs2 inet=inet2 } in_dev=subs1:subs2 out_dev=inet1:inet2

Further settings are made depending on which components are to be used. The settings are described in the SSG components section.

Implementation scheme