DHCP Server

The component is activated in a scenario with a local DHCP server. We recommend using Kea DHCP server.

It is also possible to use SSG in:

DHCP-relay — redirect requests to a specific server

DHCP RADIUS proxy mode — information about the settings is transmitted in RADIUS responses, and SSG acts as a DHCP server.