Work within the GRE/PPTP/L2TP/IPIP tunnels

Dpi doesn't parse the tunnels 1) tagged VLAN/QINQ and MPLS traffic are not considered as tunnel , since the traffic of different operators or clients with a conflicting IPs can be transmitted, but for non-standard connection (before BRAS), tunneling parsing is necessary.