Monitoring traffic distribution by class

SSG allows traffic distribution by class to be monitored.

1. Enable traffic prioritization. For the example, we will use the following prioritization rules:

dns cs0 http cs0 https cs0 Bittorrent cs7 ICMP cs0 TCP Unknown cs7 GOOGLEVIDEO cs1 default cs2

2. In the /etc/dpi/fastdpi.conf configuration, set the parameter:

dbg_log_mask=0x4

3. Enable common channel polysync (the example shown is polysync with full channel width restriction):

htb_inbound_root=rate 1300mbit htb_inbound_class0=rate 8bit ceil 1300mbit htb_inbound_class1=rate 8bit ceil 1300mbit htb_inbound_class2=rate 8bit ceil 1300mbit htb_inbound_class3=rate 8bit ceil 1300mbit htb_inbound_class4=rate 8bit ceil 1300mbit htb_inbound_class5=rate 8bit ceil 1300mbit htb_inbound_class6=rate 8bit ceil 1300mbit htb_inbound_class7=rate 8bit ceil 1300mbit htb_root=rate 1300mbit htb_class0=rate 8bit ceil 1300mbit htb_class1=rate 8bit ceil 1300mbit htb_class2=rate 8bit ceil 1300mbit htb_class3=rate 8bit ceil 1300mbit htb_class4=rate 8bit ceil 1300mbit htb_class5=rate 8bit ceil 1300mbit htb_class6=rate 8bit ceil 1300mbit htb_class7=rate 8bit ceil 1300mbit

4. Update the configuration:

service fastdpi reload
If polyscing for a shared channel is applied for the first time, you must restart the service: service fastdpi restart

5. Use the following custom settings for the zabbix agent installed on the SSG: ssg_userparams.conf

6. Import the template to the Zabbix server as described in the section "Monitoring via SNMP agent": zbx_export_templates.xml

If necessary, change the interface names in the template and in the custom parameter file

View flow and protocol statistics

By flow

IPv4/IPv6

protocol type: 0 - IPv4, 1 - IPv6

total allocated records

a queue with a short lifespan:

occupied records

reusable

difference 3.1 - 3.2 (number of active flows)

also for the long line

also total

Example:

fdpi_ctrl stat --flow IPv4 0 6784000 834 814 20 0 0 0 834 814 20

By protocols

internal index of protocol statistics

protocol name

protocol port number
direction subs -→ inet

number of packages

volume in bytes ip total

dropped packages

dropped byte
direction inet -→ subs number of packages etc.

Example:

fdpi_ctrl stat --proto Autodetected fastdpi params : dev='em1', port=29001 connecting 94.140.198.68:29001 ... ================================ 94 'ntp' 123 0 0 0 0 91 23569 0 0 4081 'sip' 5060 0 0 0 0 2479 1170579 0 0 5812 'Bittorrent' 49165 0 0 0 0 0 0 3 495 5866 'ICMP' 65025 0 0 0 0 225 18900 0 0 5871 'TCP Unknown' 65030 0 0 0 0 41034 3448836 0 0 5880 'UDP Unknown' 65041 3900 4227600 0 0 277 24825 0 0 6000 'ARP' 65282 30 2520 0 0 30 2520 0 0 6056 'CHAMELEON' 49236 0 0 0 0 589 72475 0 0