Subscriber management

General description

Configuring the platform

Service Management

Named profiles

Information on command result

Tracking buffer reset

Support for subscribers with a single IPv4 address and an IPv6 subnet binding or with dynamically assigned IP addresses

Support for subscribers with multiple IP

Changing configuration parameters

Remote control

Output of control commands using the JSON format

bras_l2_vlan_ctl