Hardware Requirements, Installation, and Update

Minimum Hardware Requirements

FastRADIUS can be installed on a SCAT server or on a dedicated server or VM.

CPU — 2 cores

RAM — from 1 GB

SSD — 50 GB

Operating System — VEOS

Network Interface Card (NIC) — 2 ports, for SSH management (+ optional IPFIX sending) and for receiving RADIUS traffic

Installation and Update

The component is included in the standard SCAT software package. If used on the same server as SCAT, no additional installation is required.

Further updates are performed in the standard way:

yum update fastradius

Installation on a Separate Server or VM

Configure precise time synchronization via the ntpd service. NTPD configuration file: /etc/sysconfig/ntpd. To do this, install the precise time service

yum install chrony -y
systemctl restart chronyd
timedatectl

When running the timedatectl command, the System clock synchronized parameter must have the value yes

Connect the vasexperts repository

rpm --import http://vasexperts.ru/centos/RPM-GPG-KEY-vasexperts.ru
rpm -Uvh http://vasexperts.ru/centos/6/x86_64/vasexperts-repo-2-1.noarch.rpm

Install FastRADIUS

yum install fastradius

Verify that the service starts

service fastradius start

Enable service autostart at boot

systemctl enable fastradius