5 Description of the Subscriber Authorization scheme in L2-connected BRAS

Subscriber authorization in L2-Connected BRAS can be done in several ways:

DHCP Radius Proxy, in this case, authorization is requested from RADIUS using the FastPCRF component

DHCP Radius Proxy + ARP authorization

DHCP Relay Agent + L3 authorization