3 L2-Connected BRAS subscriber traffic termination options

Subscriber Traffic Termination Options

The VAS Experts DPI L2-Connected BRAS can be used in schemes using IPoE and PPoE.

IPoE

The VAS Experts DPI BRAS works with the Subscribers through standard Ethernet frame exchange in the IPoE mode.

IPoE is the preferred option of the VAS Experts DPI BRAS for new installations.

PPoE

The VAS Experts DPI BRAS works with the Subscribers through PPoE encapsulation in PPoE mode.

The PPoE option is preferable to use when migrating from other BRAS devices and the IPoE option of terminating Subscriber traffic cannot be used.