SWm Authorization Interface Settings

Section "fast-epdg.auth.swm"

Parameter	Description	Value
realm	Serviced realm	epc.mncYYY.mccXXX.3gppnetwork.org
host	Client hostname	epdg.epc.mncYYY.mccXXX.3gppnetwork.org
<diameter-aaa-server-name-1> {}	AAA Server #1 parameters
<diameter-aaa-server-name-2> {}	AAA Server #2 parameters
<diameter-aaa-server-name-n> {}	AAA Server #n parameters

Template:

fast-epdg { auth { interface = swm { realm = host = <server-name> {} } } }

Example:

fast-epdg { auth { interface = SWm swm { realm = epc.mnc002.mcc250.3gppnetwork.org host = epdg.epc.mnc002.mcc250.3gppnetwork.org <server-name> {} } } }

Section "fast-epdg.auth.swm.<diameter-aaa-server-name-n>"

Parameter	Description	Value
priority	Balancing priority	0-100
local	Client address:port	AAA.BBB.CCC.DDD:XXXX, [1111.2222.3333.4444.5555.6666.7777.8888]:XXXX
remote	AAA server address:port	AAA.BBB.CCC.DDD:XXXX, [1111.2222.3333.4444.5555.6666.7777.8888]:XXXX
proto	Transport protocol	[sctp][tcp]

Template:

fast-epdg { auth { interface = swm { realm = host = diameter-aaa-server-1 { priority = local = remote = proto = } diameter-aaa-server-2 { priority = local = remote = proto = } } } }

Example:

fast-epdg { auth { interface = SWm swm { realm = epc.mnc002.mcc250.3gppnetwork.org host = epdg.epc.mnc002.mcc250.3gppnetwork.org diameter-aaa-server-1 { priority = 50 local = 192.168.1.1:3868 remote = 192.168.2.1:3868 proto = sctp } diameter-aaa-server-2 { priority = 50 local = 192.168.1.1:3869 remote = 192.168.2.2:3868 proto = tcp } } } }