Configuration of the SWu Interface

Section "fast-epdg.swu.<connection-name>"

Parameter	Description	Value
apn	Served APN	ims
leftsubnet	Network serviced by the server	IPv4: x.x.x.x/m, where x — a decimal number from 0 to 255, m — the subnet mask, a decimal number from 0 to 32 IPv6: y:y:y:y:y:y:y:y/n, where y — a hexadecimal number from 0000 to FFFF, n — the subnet mask, a decimal number from 0 to 128

Template:

fast-epdg { swu { <config-name> { apn= leftsubnet= } } }

Example:

fast-epdg { swu { <config-name> { apn=ims leftsubnet=10.0.0.0/8 } } }