Licensing

Stingray Service Gateway (SSG) liceinsing depends on the bandwidth and its features.

The license is time-unlimited.

Technical support is not included in the license and is paid separately.

SSG licensing

Bandwidth

Licenses grading of the bandwidth: SSG-6/10/20/40/60/80/100/120/200. Pay attention to the hardware requirements!
Depending on the installation scheme, the following restrictions are assumed:

1. When installing "in line" scheme

SSG-6 corresponds to 5Gb/s of incoming and to 1Gb/s of outgoing traffic

SSG-10 corresponds to 8Gb/s of incoming and to 2Gb/s of outgoing traffic

SSG-20 corresponds to 15Gb/s of incoming and to 5Gb/s of outgoing traffic

SSG-40 corresponds to 30Gb/s of incoming and to 10Gb/s of outgoing traffic

SSG-60 corresponds to 45Gb/s of incoming and to 15Gb/s of outgoing traffic

SSG-80 corresponds to 60Gb/s of incoming and to 20Gb/s of outgoing traffic

SSG-100 corresponds to 75Gb/s of incoming and to 25Gb/s of outgoing traffic

SSG-120 corresponds to 90Gb/s of incoming and to 30Gb/s of outgoing traffic

Licensing includes ISP traffic asymmetry. Usually, the incoming traffic is three times more than the outgoing one. For example, Incoming - 6G, Outgoing - 2G. License - SSG-10.

2. When installing using the "mirror" scheme

SSG-6 corresponds to 6Gb/s of total incoming traffic

SSG-10 corresponds to 10Gb/s of total incoming traffic

SSG-20 corresponds to 20Gb/s of total incoming traffic

SSG-40 corresponds to 40Gb/s of total incoming traffic

SSG-60 corresponds to 60Gb/s of total incoming traffic

SSG-80 corresponds to 80Gb/s of total incoming traffic

SSG-100 corresponds to 100Gb/s of total incoming traffic

SSG-120 corresponds to 120Gb/s of total incoming traffic

Features

Licenses grading of the features: Base/BNG/Complete

Options	BASE	BNG	COMPLETE
Bypass
Statistics gathering and analysis on protocols and directions
Traffic prioritization depending on protocols and directions
Common and virtual channel policing
Subscriber notification and marketing campaigns
Subscriber channel policing for IPv4 and IPv6
Allow Lists and Captive Portal
BNG L3 (IPoE), Dual Stack IPv4/IPv6, Radius with CoA
BNG L2 (PPPoE, DHCP), Dual Stack IPv4/IPv6
Router with BGP, OSPF, IS-IS support
Carrier-Grade NAT
Ads blocking and replacing
Mini-Firewall for blocking on certain ports
Protection against DOS and DDOS attacks
Regulatory Compliance	BASE	BNG	COMPLETE
Filtering by the blocklisted Internet sites
Lawful interception (LI)
Additional modules and services	BASE	BNG	COMPLETE
URL Classifier Local version
URL Classifier Cloud version
Graphical User Interface Base version
Graphical User Interface Global version
Quality of Experience Module Base version
Quality of Experience Module Standard version
Adding banners to HTTP resorses	Subscription
Signatures SDK	Subscription
Extended signatures packs	Subscription
Reserve License	BASE	BNG	COMPLETE
Stand by License	25% from main License

Yes
Optional
No

License Exceeding

If the license bandwidth parameters are exceeded, the DPI will process the traffic until its capabilities are exhausted. After that, traffic will be skipped without processing. You can limit the bandwidth yourself using channel policing. This is only relevant if the total bandwidth over the ports exceedes the license bandwidth specification.

Reserve SSG license

For the purpose of increasing the fault tolerance of the solution, we recommend backing up the main SSG server. Redundancy schemes and descriptions for BRAS L3 and BRAS L2.
Terms of use of the reserve license:

Use only for backup purposes of the main server

Constant traffic transmission no more than 5% of the license volume, in order to monitor the health of the backup server

Processing of all traffic of the main server only in case of an accident or maintenance of the main server

QoE licensing

Options	BASE	STANDARD
DPI’s Full NetFlow and ClickStream statistics visualization
Built-in reports of Full NetFlow-based TOP: high RTT, by traffic volume, by number of re-requests, by application protocols, by AS, by subscribers AS, by access switches and aggregation
Built-in ClickStream-based TOP reports: URLs, hosts, subscribers, devices, IP resources
Custom filters for built-in reports, by web resource category, by protocol group, by subscriber
Download reports in .xlsx, .csv, .pdf, .png formats
API support for integration with external systems
Monitoring of aplink quality and cyber threats
Online reports by specific IP, Login
NAT Flow statistics collection, compression, custom filters
DNS Flow statistics collection, compression, custom filters
GTP Flow statistics collection, compression, custom filters, map visualization
Setting triggers and actions on events, DDoS and BotNet detection, notification by email and telegram with a specified periodicity
Special reports

Yes
Optional