Licensing

Stingray Service Gateway (SSG) liceinsing depends on the bandwidth and its features.

The license is time-unlimited.

Technical support is not included in the license and is paid separately.

SSG licensing

Bandwidth

Licenses grading of the bandwidth: SSG-6/10/20/40/60/80/100/120/240. Pay attention to the hardware requirements!
Depending on the installation scheme, the following restrictions are assumed:

1. When installing "in line" scheme

SSG-6 corresponds to 6Gbps total (upload+download) traffic

SSG-10 corresponds to 10Gbps total (upload+download) traffic

SSG-20 corresponds to 20Gbps total (upload+download) traffic

SSG-40 corresponds to 40Gbps total (upload+download) traffic

SSG-60 corresponds to 60Gbps total (upload+download) traffic

SSG-80 corresponds to 80Gbps total (upload+download) traffic

SSG-100 corresponds to 100Gbps total (upload+download) traffic

SSG-120 corresponds to 120Gbps total (upload+download) traffic

SSG-120 corresponds to 240Gbps total (upload+download) traffic

Licensing includes ISP traffic asymmetry. Usually, the incoming traffic is three times more than the outgoing one. For example, Incoming - 6G, Outgoing - 2G. License - SSG-10.

2. When installing using the "mirror" scheme

SSG-6 corresponds to 6Gbps of total mirror traffic

SSG-10 corresponds to 10Gbps of total mirror traffic

SSG-20 corresponds to 20Gbps of total mirror traffic

SSG-40 corresponds to 40Gbps of total mirror traffic

SSG-60 corresponds to 60Gbps of total mirror traffic

SSG-80 corresponds to 80Gbps of total mirror traffic

SSG-100 corresponds to 100Gbps of total mirror traffic

SSG-120 corresponds to 120Gbps of total mirror traffic

Features

Licences grading of the features: Base/BNG/Complete

Options	BASE	BNG	COMPLETE
Bypass
Statistics gathering and analysis on protocols and directions
Traffic prioritization depending on protocols and directions
Common and virtual channel policing
Subscriber notification and marketing campaigns
Subscriber channel policing for IPv4 and IPv6
Allow Lists and Captive Portal
BNG L3 (IPoE), Dual Stack IPv4/IPv6, Radius with CoA
BNG L2 (PPPoE, DHCP), Dual Stack IPv4/IPv6
Router with BGP, OSPF, IS-IS support
Carrier-Grade NAT
Ads blocking and replacing
Mini-Firewall for blocking on certain ports
Protection against DOS and DDOS attacks
Regulatory Compliance	BASE	BNG	COMPLETE
Filtering by the blocklisted Internet sites
Lawful interception (LI)
Additional modules and services	BASE	BNG	COMPLETE
URL Classifier Local version
URL Classifier Cloud version
Graphical User Interface Base version
Graphical User Interface Global version
Quality of Experience Module Base version
Quality of Experience Module Standard version
Adding banners to HTTP resorses	Subscription
Signatures SDK	Subscription
Extended signatures packs	Subscription
Reserve License	BASE	BNG	COMPLETE
Stand by License	25% from main License

Yes
Optional
No

License Exceeding

If the bandwidth license parameters are exceeded, SSG will process traffic until the platform reserves are exhausted. Once the platform capacity is exhausted, processing errors will occur and traffic degradation will occur. You can limit the bandwidth yourself by polysizing: Common and Virtual Channels Policing, this is only relevant when the total port throughput exceeds the license bandwidth parameters.

VAS Experts reserves the right to refuse technical support or project maintenance to customers who do not comply with license terms, including those who exceed the allowed traffic (including according to the built-in error monitoring system).

Reserve SSG license

For the purpose of increasing the fault tolerance of the solution, we recommend backing up the main SSG server. Redundancy schemes and descriptions for BRAS L3 and BRAS L2.
Terms of use of the reserve license:

Use only for backup purposes of the main server

Constant traffic transmission no more than 5% of the license volume, in order to monitor the health of the backup server

Processing of all traffic of the main server only in case of an accident or maintenance of the main server

QoE licensing

Options	BASE	STANDARD
DPI’s Full NetFlow and ClickStream statistics visualization
Built-in reports of Full NetFlow-based TOP: high RTT, by traffic volume, by number of re-requests, by application protocols, by AS, by subscribers AS, by access switches and aggregation
Built-in ClickStream-based TOP reports: URLs, hosts, subscribers, devices, IP resources
Custom filters for built-in reports, by web resource category, by protocol group, by subscriber
Download reports in .xlsx, .csv, .pdf, .png formats
API support for integration with external systems
Monitoring of aplink quality and cyber threats
Online reports by specific IP, Login
NAT Flow statistics collection, compression, custom filters
DNS Flow statistics collection, compression, custom filters
GTP Flow statistics collection, compression, custom filters, map visualization
Setting triggers and actions on events, DDoS and BotNet detection, notification by email and telegram with a specified periodicity
Special reports

Yes
Optional