10 Licensing

VAS Experts DPI liceinsing depends on the bandwidth and its features:

Bandwidth

Licenses grading of the bandwidth: VAS Experts DPI DPI-6/10/20/40/60/80/100
Depending on the installation scheme, the following restrictions are assumed:

When installing "in the gap" scheme

VAS Experts DPI-6 corresponds to 3Gb/s of incoming and to 3Gb/s of outgoing traffic

VAS Experts DPI-10 corresponds to 5Gb/s of incoming and to 5Gb/s of outgoing traffic

VAS Experts DPI-20 corresponds to 10Gb/s of incoming and to 10Gb/s of outgoing traffic

VAS Experts DPI-40 corresponds to 20Gb/s of incoming and to 20Gb/s of outgoing traffic

VAS Experts DPI-80 corresponds to 40Gb/s of incoming and to 40Gb/s of outgoing traffic

VAS Experts DPI-100 corresponds to 50Gb/s of incoming and to 50Gb/s of outgoing traffic

The license is determined by the formula max(in,out)*2

When installing using the "mirror" scheme

VAS Experts DPI-6 corresponds to 6Gb/s of total incoming traffic

СКАТ DPI-10 corresponds to 10Gb/s of total incoming traffic

СКАТ DPI-20 corresponds to 20Gb/s of total incoming traffic

СКАТ DPI-40 corresponds to 40Gb/s of total incoming traffic

СКАТ DPI-80 corresponds to 80Gb/s of total incoming traffic

СКАТ DPI-100 corresponds to 100Gb/s of total incoming traffic

Features

Licenses grading of the features: Enty/Base/Complete

Превышение параметров лицензии

При превышении параметров лицензии по полосе DPI будет обрабатывать трафик до пределов пока заложенные резервы не будут исчерпаны, по их исчерпанию трафик будет пропущен без обработки. Ограничить полосу можно самостоятельно с помощью полисинга канала, это актуально только при превышении суммарной полосы по портам над параметрами полосы лицензии.