Next set of parametrers can be given from DPI:

Errors in logs of fastdpi /var/log/dpi/fastdpi_alert.log

Errors in system log /var/log/messages

Drops on dna devices

Device traffic volume

State of control devices

Quantity of processed requests for HTTP, HTTPS

Quantity of locked requests for HTTP, HTTPS, IP

Zabbix Agent is used in the example.

1. Zabbix Agent installation:

rpm -ivh http://repo.zabbix.com/zabbix/2.4/rhel/6/x86_64/zabbix-release-2.4-1.el6.noarch.rpm
yum install zabbix-agent

2. Change SELinux policy

yum update selinux-policy

3. Put skat_userparams.conf into directory: /etc/zabbix/zabbix_agent.d/ and zabbix_agentd.conf into /etc/zabbix/

4.Edit file /etc/zabbix/zabbix_agentd.conf:

Server=%address of zabbix server%
ServerActive=%address of zabbix server%
Hostname=%servers' hostname%

5. Change file context /var/log/dpi/fastdpi_stat.log:

chcon unconfined_u:object_r:zabbix_log_t:s0 /var/log/dpi/fastdpi_stat.log

6. add into /etc/sysconfig/iptables the rule before -A INPUT -j REJECT:
-A INPUT -p tcp --dport 10050 -j ACCEPT

7. Reload iptables:

service iptables reload

7. Make agent start at reboot and run it:

chkconfig zabbix-agent on
service zabbix-agent start

8. import DPI template into Zabbix zbx_template_dpi.xml. In the management pannel of Zabix server insert a new host and link it to the imported template.

9. In Zabix GUI set off requests to network devices that isn't used in DPI - click on enabled from right