This service is configured on individual subscribers' level by fdpi_ctrl.

Instruction format:

fdpi_ctrl command --service 6 [IP_list]

You can find more details on the instruction syntax and IP specification methods here: Control instructions

Examples:

To activate notification for a particular subscriber:

fdpi_ctrl load --service 6 --ip 192.168.0.1

After successful notification the service is switched off automatically.