To make it possible for the DPI platform to receive SM control commands, one has to specify the following settings in its configuration file /etc/dpi/fastdpi.conf:

The listening port number:

ctrl_port=29000

The network interface name:

ctrl_dev=eth0