3 Use cases

Stingray Service Gateway Server

Before installing VEOS, the server hardware must be prepared according to the instructions in the Stingray SG section.

To configure the operating mode of the DPI server after a successful installation and VEOS boot, the OS must be preconfigured.