This service is configured for individual subscribers by fdpi_ctrl.

Instruction format:

fdpi_ctrl command --service 5 [список_IP]

The instruction syntax and IP addresses specification methods are described in details here: Control instructions.

Examples:

Enable the "white list" operation for the particular subscriber:

fdpi_ctrl load --service 5 --ip 192.168.0.1

Disable the "white list" operation for the particular subscriber:

fdpi_ctrl del --service 5 --ip 192.168.0.1