Version 7.0 Minsk

The main changes to the 7.0 verison Minsk1) Minsk is a hero-city, now represents an important role in the peace process, many of our good customers are from this fair city

Initial IPv6 support ( filtering, protocol recognition, metadata export, netflow v10 export)

New features L2 BRAS ( VLAN/QinQ termination, DHCP relay, IP Source Guard) are added

DHCP-Radius gateway, enabling to request DHCP settings through the Radius server without the DHCP server, is added

Radius Accounting is added

The GRE tunneling support via the built-in NAT (PPTP/GRE ALG) is added

Changes to the 7.1 version

Fragmented traffic detection and handling, including the http/https recognition feature are improved

Bugs in L3 BRAS and Radius CoA revealed at the software implementation are fixed

Bug in the database engine intended to handle bind_multi are fixed

Changes to the 7.2 version

The support of NAT 1:1 is added

The support of PPPoE termintaion in L2 BRAS is added

Bugs in BRAS operation revealed at the software implementation are fixed

Changes to the 7.3 version

The memory consumption when using NAT is reduced

Improvements to the CGNAT are made

New configuration options nat_exclude_private and nat_private_cidr are added

The metadata export of http response

Changes to the 7.4 version

Bug revealed when using NAT service of higher (multi-cluster) versions is fixed

htb descriptors leakage in case of frequent policing changes regarding bind_multi subscribers

Revisions and additions to L2 BRAS operation по результатам внедрений

Изменения в версии 7.5

Service 12 - write the subscriber's traffic to a PCAP file

The possibility of applying the CoA using the Acct-Session-Id (is used when the Framed-IP-Address or User-Name aren't specified) is added

User-Name и VasExperts-NAT-IP attributes are added to accounting

Idle-Timeout support is added to all types of authentication

STUN signature is fixed

Metadata export for the OSCAR/ICQ protocol is fixed

In order to check the currently installed version enter the command

yum info fastdpi

Downgrade to 7.4 version:

yum downgrade fastdpi-7.4

After updating or downgrading, a service restart is required:

service fastdpi restart

Do not upgrade the Linux kernel. In the new version of kernel-2.6.32-431.29.2 or later, binary compatibility with Kernel ABI is broken and the network driver will not boot after the update. If you already have upgraded, then at the time of solving the problem, please configure the grub boot loader to load the previous kernel version (in the /etc/grub.conf file set default=1).

To check the changes in the previous version.