Equipment prerequisites

Minimum requirements

You can use equipment or virtual machines within the subsystem with the following characteristics:

Central Processor Unit (CPU) — 2.5 GHz, 1 pce

Random access memory (RAM) — 2 GB min

Hard disk drive (HDD) — 50 - 250 GB

Operating System — CentOS 8.x, VEOS, CentOS Stream 8.x, Oracle Linux Server 8.x, AlmaLinux 8.x.
When using VEOS, take into account the information in VEOS Update Notes when selecting hardware.

Network interface card (NIC) — 10 Mbps and above

Recommended requirements

Central Processor Unit (CPU) — 2 - 4 cores, 1 pce

Random access memory (RAM) — 4 - 8 GB

SSD — 100 GB

Operating System — CentOS 8.x, VEOS, CentOS Stream 8.x, Oracle Linux Server 8.x, AlmaLinux 8.x.
When using VEOS, take into account the information in VEOS Update Notes when selecting hardware.

Network interface card (NIC) — 10 Mbps and above

Do not install the subsystem on the same hardware with the DPI! Use a separate virtual machine instead.
The GUI can synchronize a maximum of 300,000 subscribers with the DPI.