Test version installation

Here is the translation with formatting preserved:

Changes in version 13.2 BETA1

[BRAS][PPPoE] Fixed: ping of inactive client with Echo requests

Support for service profiles 19 (DNS response substitution). Description

For service 19, ability to specify AAAA records and support for wildcard (*) for domains. Description

Fixed: for profile 18, it is not required to set both DSCP and TBF simultaneously

Changes in Version 13.2 BETA2

Fixed: IP:PORT priority over IP and CIDR for custom protocol definitions

Modified: custom protocols have higher priority than cloud protocols

Fixed: length of AAAA records in service 19

Added: mask 8 in block_options - do not generate rst blocking and redirection packets for packets directed from inet-→subs

Changes in version 13.2 BETA3

[DPI] Improved: analysis of out-of-order packets.

[DPI] Fixed: recognition of DOT protocol.

[CTRL] Added: new format for policing output:

fdpi_ctrl list profile --policing --profile.name htb_6 --outformat=json2

.

[CTRL] Added: loading of policing profiles with the new format (including value and unit).

[BRAS][IPv6] Added: upon receiving a DHCPv6 confirm from the client and if there is no session in the BRAS database, a response with the status "NotOnLink" is sent.

[FastPCRF][DHCPv6] Fixed: an error causing the current IPv6 accounting session to close and reopen when processing DHCPv6 requests from the client to renew the address lease.

Update instructions

You can check the current installed version with the command below

yum info fastdpi

If you have CentOS 6.x or CentOS 8.x installed, then switch the repository once with the command:

sed -i -e '/^mirrorlist=http:\/\//d' -e 's/^# *baseurl=http:\/\/mirror.centos.org/baseurl=http:\/\/vault .centos.org/' /etc/yum.repos.d/CentOS-*.repo

and then update as usual.

To install the test version, you should issue the following command:

yum --enablerepo vasexperts-beta update fastdpi

Downgrade to 13.1:

yum downgrade fastdpi-13.1 fastpcrf-13.1
After an update or version change, a restart of the service is required.