13 SCAT-80/CISCO SCE 10000

VASEXPERTS SCAT-80	CISCO SCE10000
Technology	data streams distribution on multi-core CPU Intel x86 Programmable extensible architecture that provides investment protection
Throughput	80 Gbit/s 2,5 Gbit/s in cluster	60 Gbit/s 480 Gbit/s in cluster
Maximum No. of sessions	80 mln	20 mln
Subscribers	8 млн	2 млн
Hardware: RAM, CPU, Hard Drive, Main Network, Control Network	128 GB, CPU 18 cores HDD 2 x 500 GB 8 x 10 GBE с bypass 1 x 1GBE	512 GB, CPU 40 cores HDD 2 x 300 GB 8 x 10 GBE с bypass 4 x 1 GBE
Size	1 Rack Unit	2 Rack Unit
Min GPL Price	20 000 usd	400 000 usd