2 Installation

Initial installation of Radius events monitor is handled by tech support engineers of VAS Experts company or its partners.

You have to install OS CentOS 6.5 before the implementation. Please provide us the remote access by SSH and root rights. This access is required for installation and initial setup of the platform. The remote access can be closed after finishing the installation works.

Further updates are carried out in a standard way:

yum update fastradius