General description

The bandwidth control for subscribers is similar to the overall bandwidth control. All options are available:

Bandwidth limitation by the traffic classes (for example: limit torrents

Traffic's prioritization within the subscriber's bandwidth with borrowing (HTB) or as "pipes" (TBF)

The assignment of traffic control policies for subscribers is supported by Subscriber Management,SM.

This option eliminates using BRAS for operators who use IPoE technology for subscribers' connections.