6 Troubleshooting

Flow sending is configured today, but an issue emerges - not all the information are transmitted. We have completed simple test - download the file from the network, the received data are much less than the downloaded ones of 700MB/2,5MB using 2Gb network interface as a NetFlow collector, peak load is about 20Mbit. How to fix the problem?

We have an experiment with the netflow_timeout option. With the netflow_timeout = 1 no data loss.

How to generate a time report in format suitable for opening in Excell?