Development Plans

Development Plans for 2023

BRAS/BNG

Release of the version with On-Stick support with port dividing by VLAN-ID

Release of the version with support for aggregation of ports into LAG by Stingray

Single Session support for IPv4/IPv6

Support for Active-Active and Active-Standby redundancy scheme for BRAS DHCP

Support of subscriber quota and logic for switching tariff plan in case of quota exhaustion, depending on time of day (based on PCRF logic).

Creation of dynamic service interfaces (access points) for Dot1Q, Q-in-Q ranges with the ability to specify connection types for each range

Host Lockout support - Functionality that allows to block attempts of a subscriber to connect (not to send an authorization request to the Radius server) in case of repeated failure of authorization

Use of different Radius groups for authentication

L3VPN implementation

L2TP support

Supports MPLS label-based routing. LDP protocol and segment routing

DPI

Support for different prefix lengths for IPv6 (now only fixed size /64 or /56 or /48 is supported)

Development of custom signatures service

Redirecting traffic according to specified criteria, for example, DNS spoofing. The criteria will be port, protocol. Redirection is performed in VLAN on Linux interface with balancing

DSCP tag mapping

Implementation of ACL analog

NAT

NAT 64, will allow to use a single IPv6 stack and avoid routing table overflow

More

Support for 5G core network

Diameter protocol support (Gx, Gy, Gz interfaces)

Development of services: DDoS, Botnet, SPAM detection.