S2b Tunneling Interface Settings

Section "fast-epdg.tunnel"

Parameter	Description	Value
iface	Used interface	[sgw][epdg]
pdn	PDN type	[ipv4][ipv6][ipv46]
pgw {}	S2b interface settings

Template:

fast-epdg { tunnel { iface = pdn = pgw {} } }

Example:

fast-epdg { tunnel { iface = epdg pdn = ipv4 pgw {} } }