The remote execution of SSH commands is the recommended method to control DPI from another computer. Billing systems typically have the built in support of this control method.

The alternative remote control methods are: remote execution of fdpi_ctrl utility and installation of an additional remote control SW on DPI server, like telnet server, snmp agent and similar.